*version 9.2 711462644
@index
symloc vdb 0 384
symloc idb 384 386
symloc vphase 770 378
symloc iphase 1148 380
symloc vgroupdelay 1528 389
symloc igroupdelay 1917 391
symloc vreal 2308 381
symloc ireal 2689 383
symloc vimaginary 3072 391
symloc iimaginary 3463 393
symloc IMARKER 3856 374
symloc NODEMARKER 4230 341
symloc VDIFFMARKER 4571 376
symloc copyright 4947 601
*symbol vdb
d db magnitude of voltage
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
a 0 u 0 0 0 10 hlb 100 FUNCTION=VDB
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 16 12 hln 50 VDB
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol idb
d db magnitude of current
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
a 0 u 0 0 0 10 hlb 100 FUNCTION=DB
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 16 12 hln 50 IDB
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol vphase
d phase of voltage
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
a 0 u 0 0 0 10 hlb 100 FUNCTION=VP
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 16 12 hln 50 VP
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol iphase
d phase of current
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
a 0 u 0 0 0 10 hlb 100 FUNCTION=P
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 50 IP
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol vgroupdelay
d group delay of voltage
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
a 0 u 0 0 0 10 hlb 100 FUNCTION=VG
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 16 12 hln 50 VG
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol igroupdelay
d group delay of current
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
a 0 u 0 0 0 10 hlb 100 FUNCTION=G
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 50 IG
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol vreal
d real part of voltage
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
a 0 u 0 0 0 20 hlb 100 FUNCTION=VR
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 16 12 hln 50 VR
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol ireal
d real part of current
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
a 0 u 0 0 0 10 hlb 100 FUNCTION=R
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 50 IR
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol vimaginary
d imaginary part of voltage
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
a 0 u 0 0 0 10 hlb 100 FUNCTION=VI
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 50 VI
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol iimaginary
d Imaginary part of current
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
a 0 u 0 0 0 10 hlb 100 FUNCTION=I
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 50 II
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol IMARKER
d Current marker
@type e
@attributes
a 0 s 0 0 6 20 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=CURRENT
@pins
p 0 12 34 hln 100 pin1 z 0 30 h
a 0 u 0 0 1 30 hln 100 pin=1
a 0 u 0 0 0 32 hln 100 ERC=x
@graphics 30 30 0 30 10
c 0 20 10 5
v 0 20 7
20 12
;
v 0 18 7
22 7
;
v 0 18 12
22 12
;
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol NODEMARKER
d Node marker
@type e
@attributes
a 0 s 0 0 4 22 hlb 100 LABEL=?
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=NODE
@pins
p 0 11 31 hln 100 pin1 z 0 30 h
a 0 u 0 0 0 27 hln 100 pin=1
a 0 u 0 0 -1 29 hln 100 ERC=x
@graphics 30 30 0 30 10
s 26 18 12 hln 75 V
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol VDIFFMARKER
d Voltage differential marker
@type e
@attributes
a 0 s 0 0 6 20 hlb 100 LABEL=?
a 0 s 13 0 16 14 hlb 100 NODE=+
a 0 s 0 0 0 10 hlb 100 MARKERTYPE=VOLTAGEDIFF
@pins
p 0 12 33 hln 100 pin1 z 0 30 h
a 0 u 0 0 1 29 hln 100 pin=1
a 0 u 0 0 0 31 hln 100 ERC=x
@graphics 30 30 0 30 10
c 0 20 10 5
v 0 0 30
4 22
;
v 0 4 22
8 26
;
v 0 8 26
0 30
;
v 0 6 24
17 13
;
*symbol copyright
d Copyright
@type p 9.2
@attributes
a 0 sp 9 0 0 0 hln 100 REFDES=U?
a 0 sp 11 0 0 70 hln 100 PART=
a 0 sp 0 0 0 0 hln 100 MODEL=
a 0 sp 0 0 0 0 hln 100 TEMPLATE=
@pins
@graphics 230 60 0 0 10
r 0 0 0 230 60
z 26 2 10 hln 100 43
Copyright 2000 Cadence Design Systems, Inc.
z 26 2 38 hln 100 41
Neither this library, nor any part of it,
z 26 2 47 hln 100 41
may be copied without the express written
z 26 2 57 hln 100 39
consent of Cadence Design Systems, Inc.
z 26 2 29 hln 100 35
the PSpice Schematics program only.
z 26 2 20 hln 100 44
The symbols in this library are for use with
