Protel Design System Design Rule Check
PCB File : VAG.PCB
Date     : 28-Feb-2005
Time     : 10:40:30

Processing Rule : Clearance Constraint (Gap=0.254mm) (Disabled)(On the board ),(On the board )
Rule Violations :0

Processing Rule : Clearance Constraint (Gap=0.508mm) (Is a Polygon  ),(On the board )
Rule Violations :0

Processing Rule : Room VAG (Region = (569.849mm, 115.697mm, 620.649mm, 166.497mm) (Disabled)(Is part of Component class VAG )
Rule Violations :0

Processing Rule : Width Constraint (Min=0.254mm) (Max=0.254mm) (Prefered=0.254mm) (Disabled)(On the board )
Rule Violations :0

Processing Rule : Width Constraint (Min=0.254mm) (Max=2.54mm) (Prefered=0.508mm) (On the board )
Rule Violations :0

Processing Rule : Hole Size Constraint (Min=0.0254mm) (Max=2.54mm) (On the board )
Rule Violations :0

Processing Rule : Broken-Net Constraint ( (On the board ) )
Rule Violations :0

Processing Rule : Short-Circuit Constraint (Allowed=Not Allowed) (On the board ),(On the board )
Rule Violations :0


Violations Detected : 0
Time Elapsed        : 00:00:01
